1. Number of nodes = 149

Number of Zones = 41

1. Speed Limit = 39 mph

Number of lanes = 2 lanes

1. Link capacity is the capacity for multiple lanes while Lane capacity is the capacity of a single lane.
2. The link capacity for S Redwood Rd is (2562) between nodes 5436 through 11160, and then it decreases to 1784 between nodes 11172 to 5112. Also it then decreases again to (929) between nodes 5238 to 5208
3. The number of agents/vehicles as reported in the output summary is 25282 vehicles.
4. Average travel time = 16.0217 minutes

Average Trip Time Index = 2.97

Average speed = 11.3456

Network clearance time = 1350 minutes

I was not able to get the work zone file to work on my laptop and the link MOE tool was not visible either